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Figure a) Scheme of Na-CO2 battery with La0.7Sr0.3Mn1-xNixO3 catalyst (LSMN) in the cathode, b) in-situ Raman spectrum of a Na-CO2 battery composed of the La0.7Sr0.3Mn0.5Ni0.5 catalyst.
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