**NZTA T24: 2025 Procedure To Determine the Plateau Dry Density**

Presenters: Rob Damhuis (Waka Kotahi NZTA) & Thorsten Frobel (Downer Group)

Since 2005, NZTA has required Plateau Density tests in their B-series specifications. However, no standard methodology was ever established, although specified. This test method is the product of over 3 years, with industry and NZTA working collaboratively to develop a standardised Plateau Density test method.

This presentation will highlight the journey, the learnings along the way, and the collaborative arrangement between contractor and laboratory needed to get the best test outcome.