**Flexible silicon carbide electronics for long-lived bio-implantable recording and sensing applications**

*Hoang-Phuong Phan,\*,†,‡ Yishan Zhong,⊥ Tuan-Khoa Nguyen,† Yoonseok Park,‡ Toan Dinh,† Enming Song,‡⊥ Raja Kumar Vadivelu,† Mostafa Kamal Masud,║ Jinghua Li,⊥,∇ Muhammad J.A. Shiddiky,†,○ Dzung Dao,†,§ Yusuke Yamauchi,║,&,∇ John A. Rogers,\*,# and Nam-Trung Nguyen\*,†*

†Queensland Micro and Nanotechnology Centre, Griffith University, Brisbane, Queensland 4111, Australia.

‡Center for Bio-Integrated Electronics, Northwestern University, Evanston, IL 60208, USA.

§School of Engineering and Built Environment, Griffith University, Gold Coast, Queensland 4215, Australia.

⊥Frederick Seitz Materials Research Laboratory, University of Illinois at Urbana-Champaign, Urbana, IL 61801, USA.

║Australian Institute for Bioengineering & Nanotechnology and School of Chemical Engineering, University of Queensland, Brisbane, Queensland 4072, Australia.

∇Department of Materials Science and Engineering, Northwestern University, Evanston, IL 60208, USA.

○School of Environment and Science, Griffith University, Brisbane, Queensland 4111, Australia.

&International Center for Materials Nanoarchitectonics (WPI-MANA), National Institute for Materials Science (NIMS), 1-1 Namiki, Tsukuba, Ibaraki 305-0044, Japan

∇Department of Plant & Environmental New Resources, Kyung Hee University, 1732 Deogyeong-daero, Giheung-gu, Yongin-si, Gyeonggi-do 446-701, Korea

#Center for Bio-Integrated Electronics, Department of Materials Science and Engineering, Biomedical Engineering, Chemistry, Mechanical Engineering, Electrical Engineering and, Computer Science, and Neurological Surgery, Simpson Querrey Institute for Nano/biotechnology, McCormick School of Engineering and Feinberg School of Medicine, Northwestern University, Evanston, IL 60208, USA.

**Abstract**

Implantable electronics are of great interest owing to their capability for real-time and continuous cellular-electrical-activity recording.1 Nevertheless, since such systems involve direct interfaces with surrounding biofluidic environments, maintaining their long-term sustainable operation, without leakage currents or corrosion, is a daunting challenge.2

In this talk, we present a new bio-integrated bioelectronics systems based on cubic silicon carbide nanomembranes grown on silicon wafers,3 released and then physically transferred to a flexible substrate.4 Our findings demonstrate that flexible platforms based on nanomembranes of SiC offer many attractive features as long-lived implantable devices owing to its chemical stability in biofluids, outstanding water barrier characteristics and extremely low permeability to ions, suitable for stable operation with projected lifetimes of many decades in biological environments. The fabrication approach to release and transfer nanomembranes SiC onto flexible polymer substrates such as PI establishes a route to systems well suited for integration with soft tissues, enabling the development of unusual wide-band-gap semiconducting devices with bendable, foldable and flexible formats and advanced functional modes. The robustness of the SiC bio-interface along with its interesting physical properties including thermoresistive, piezoresistive effects suggest a promising path toward advanced versions of long-term implantable electronics for chronic neural and cardiac electrophysiology.

**References:**

1. Someya, T.; Bao, Z; Malliaras, G.G. (2016). The Rise of Plastic Bioelectronics. Nature, 540, 379-385.
2. Rotenberg, M.Y.; Tian, B. (2017) Bioelectronic Devices: Long-Lived Recordings. Nat. Biomed. Eng., 1(3), 0048.
3. Phan, H.P., Masud, M.K., Vadivelu, R.K., Dinh, T., Nguyen, T.K., Kieu, N.G.O., Dao, D., Shiddiky, M.J., Hossain, M.S., Yamauchi, Y. and Nguyen, N.T. (2019). Transparent crystalline cubic SiC-on-glass electrodes enable simultaneous electrochemistry and optical microscopy. Chem. Comm., 55, 7978-7981.
4. Phan,H-P., Zhong, Y.; Nguyen, T.-K.; *et al.* (2019) Long-Lived, Transferred Crystalline Silicon Carbide Nanomembranes for Implantable Flexible Electronics, ACS Nano. *In press*.